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HEALTH & SAFETY DATA SHEET

CONCRETE PRODUCTS 

PRODUCT

Concrete products are designed to enable the user to construct structures in accordance with individual product specifications

PHYSICAL AND CHEMICAL CHARACTERISTICS

Concrete products are manufactured to fine tolerances by the compaction of a hydrated mixture of aggregates and cementitious materials that subsequently undergo a curing process

MAIN HAZARDS

Handling of concrete products may cause abrasive damage to the hands. Excessive handling may cause dermatitis or drying of unprotected skin. Cutting or similar surface treatment of the products will give rise to respirable dust. Such dust, if inhaled in excessive quantities over extended periods, can constitute a long-term health hazard. Cutting, drilling, chasing, etc., unless adequately controlled, can project particles at high velocity with consequent risk of impact damage.

PRECAUTIONS

During cutting or similar surface treatment, inhalation of dust must be avoided, and eyes must be protected.

PROTECTIVE EQUIPMENT

Whilst handling, protective gloves should be worn. During cutting or similar activity, goggles should be worn, as should ear and respiratory protective equipment (dust masks to BS.2091 Type B/ or equivalent). 

TRANSPORTATION, STORAGE AND DISPOSAL

The carriage of concrete products is not subject to hazardous substance conveyance regulations and vehicle labeling is not required. Concrete products are inert, but should be disposed of in accordance with local legal requirements. Particular care should be taken in the stacking and general handling of individual units or packs of units, taking into account the weight of the products, angle of repose, stability of the packs, etc.

For further information please contact S. Morris Ltd.
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